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Dear Addressee (or other typical greeting),

Rockwell Automation announces the 140A Manual motor starters / Motor Protection Circuit Breakers will be discontinued and no longer available for sale after 31 October 2020.*.

To support your transition, we recommend migrating to 140MP Motor Protection Circuit Breakers. The 140MP line offers:
· Overload protection – trip class 10A
· Short-Circuit Protection (Magnetic Protection)
· Phase loss sensitivity
· Testing in combination with Allen-Bradley Bulletin 100-C and 100-K contactors to create two component motor starters
· CE, cULus, CCC, KC, EAC Certification

Following are the products that are affected: 



	140A Catalog Number
	140A Description
	Discontinued Date*
	140MP Recommended Replacement
	140MP Description
	Replacement Category**

	140A-C2A-A16
	0.1 - 0.16 A Manual motor Starter
	10/31/2020
	140MP-A3E-A16
	140MP 0.16A Mtr Protection Ckt-br
	Engineered Replacement

	140A-C2A-A25
	0.16 - 0.25 A Manual motor Starter
	10/31/2020
	140MP-A3E-A25
	140MP 0.25A Mtr Protection Ckt-br
	Engineered Replacement

	140A- C2A -A40
	0.25 - 0.40 A Manual motor Starter
	10/31/2020
	140MP-A3E-A40
	140MP 0.40A Mtr Protection Ckt-br
	Engineered Replacement

	140A- C2A -A63
	0.4 - 0.63 A Manual motor Starter
	10/31/2020
	140MP-A3E-A63
	140MP 0.63A Mtr Protection Ckt-br
	Engineered Replacement

	140A- C2A -B10
	0.63 - 1.0 A Manual motor Starter
	10/31/2020
	140MP-A3E-B10
	140MP 1.0A Mtr Protection Ckt-br
	Engineered Replacement

	140A- C2A -B16
	1.0 - 1.6 A Manual motor Starter
	10/31/2020
	140MP-A3E-B16
	140MP 1.6A Mtr Protection Ckt-br
	Engineered Replacement

	140A- C2A -B25
	1.6 - 2.5 A Manual motor Starter
	10/31/2020
	140MP-A3E-B25
	140MP 2.5A Mtr Protection Ckt-br
	Engineered Replacement

	140A- C2A -B40
	2.5 - 4.0 A Manual motor Starter
	10/31/2020
	140MP-A3E-B40
	140MP 4.0A Mtr Protection Ckt-br
	Engineered Replacement

	140A- C2A -B63
	4.0 - 6.3 A Manual motor Starter
	10/31/2020
	140MP-A3E-B63
	140MP 6.3A Mtr Protection Ckt-br
	Engineered Replacement

	140A- C2A -C10
	6.3 - 10 A Manual motor Starter
	10/31/2020
	140MP-A3E-C10
	140MP 10A Mtr Protection Ckt-br
	Engineered Replacement

	140A- C2A -C16
	10 - 16 A Manual motor Starter
	10/31/2020
	140MP-A3E-C16
	140MP 16A Mtr Protection Ckt-br
	Engineered Replacement


 Manual motor Starter / Motor Protection Circuit Breakers

Auxiliary Contacts
	Catalog Number
	140A Description
	Discontinued Date*
	140MP Recommended Replacement
	140MP Description
	Replacement Category**

	140A-C-AEA01
	Flush mount – 1NC
	10/31/2020
	140MP-A-AFA01
	Front mount – 1NC
	Functional

	140A-C-AEA10
	Flush mount – 1NO
	10/31/2020
	140MP-A-AFA10
	Front mount – 1 NO
	Functional

	140A-C-AEA201
	Flush mount – 1NC
	10/31/2020
	140MP-A-AFA01
	Front mount – 1NC
	Functional

	140A-C-AEA210
	Flush mount – 1NO
	10/31/2020
	140MP-A-AFA10
	Front mount – 1 NO
	Functional

	140A-C-ASA02
	Side mount – 2 NC
	10/31/2020
	140MP-A-ASA02
	Side mount – 2 NC
	Functional

	140A-C-ASA11
	Side mount – 1 NO, 1 NC
	10/31/2020
	140MP-A-ASA11
	Side mount – 1 NO, 1 NC
	Functional

	140A-C-ASA20
	Side mount – 2 NO
	10/31/2020
	140MP-A-ASA20
	Side mount – 2 NO
	Functional
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Shunt Trip Release
	Catalog Number
	140A Description
	Discontinued Date*
	Recommended Replacement
	140MP Description
	Replacement Category**

	140A-C-SXD
	110V, 50 Hz/120V, 60 Hz
	10/31/2020
	140MP-A-SND
	110 V, 50/60 Hz
	Functional

	140A-C-SXF
	220-230V, 50 Hz
	10/31/2020
	140MP-A-SNAF
	200-240 V, 50/60 Hz
	Functional

	140A-C-SXJ
	24V, 60 Hz
	10/31/2020
	140MP-A-SNKJ
	20-24 V, 50/60 Hz
	Functional

	140A-C-SXK
	24V, 50 Hz
	10/31/2020
	140MP-A-SNKJ
	20-24 V, 50/60 Hz
	Functional

	140A-C-SXN
	400V, 50 Hz/460V, 60 Hz
	10/31/2020
	140MP-A-SNN
	350-415 V, 50/60 Hz
	Functional




Undervoltage Trip Release
	Catalog Number
	140A Description
	Discontinued Date*
	Recommended Replacement
	140MP Description
	Replacement Category**

	140A-C-UXB
	415V, 50 Hz/480V, 60 Hz
	10/31/2020
	140MP-A-UXB
	415V 50Hz, 480V 60 Hz
	Functional

	140A-C-UXD
	110V, 50 Hz/120V, 60 Hz
	10/31/2020
	140MP-A-UXC
	110V 50Hz, 120V 60 Hz
	Functional

	140A-C-UXF
	220-230V, 50 Hz
	10/31/2020
	140MP-A-UXF
	230V 50Hz, 240V 60 Hz
	Functional

	140A-C-UXJ
	24V, 60 Hz
	10/31/2020
	140MP-A-UXJ
	20V 50Hz, 24V 60 Hz
	Functional

	140A-C-UXK
	24V, 50 Hz
	10/31/2020
	140MP-A-UXK
	24V 50Hz, 28V 60Hz
	Functional

	140A-C-UXM
	500V, 50 Hz/575V, 60 Hz
	10/31/2020
	140MP-A-UXM
	575V 60 Hz
	Functional

	140A-C-UXN
	400V, 50 Hz/460V, 60 Hz
	10/31/2020
	140MP-A-UXN
	400V 50Hz
	Functional






Please note products may sell out prior to the discontinuation date listed above. We recommend you place all last-time buy orders as far in advance of the discontinued date as possible by contacting your local Allen-Bradley distributor or Rockwell Automation sales engineer. 


Product stocking varies globally region-to-region. Some regions may have product available for sale up to one year after a product discontinuation date. To check product availability in your region, contact your local Allen-Bradley distributor or Rockwell Automation sales engineer.


Rockwell Automation plans to provide repair services and technical support for these products for as long as practical. If you are interested in using some of these services, please contact our technical support at http://www.rockwellautomation.com/global/support/overview.page. Note that most services are chargeable and may require a technical support contract.


Migration Solutions
Rockwell Automation can help you identify your options for leveraging your existing automation investment across the enterprise and throughout the lifecycle. Use our Product Lifecycle Status search tool to find specific lifecycle information by catalog number.

As always, we will make every attempt to satisfy your needs. Please feel free to contact me with any concerns or transition issues.


<product manager’s name>
<product manager’s title>
<product manager’s contact info>


Complimentary Close,



*Discontinued date may be subject to change.
**Definition of replacement categories:
Direct Replacement: a product that can be used in place of an earlier product without any user modifications or adjustments. A direct replacement provides backward compatible form, fit and function by emulating the earlier product.

Functional Replacement: a product or family that can be used to replace an earlier product or family and emulates the old one with minimal changes to an existing application. A functional replacement means that there is a form, fit or function change, but that it is backward compatible.

Engineered Replacement: a product or family that can be used to migrate an earlier product or family and requires engineering changes to existing applications. An engineered replacement means that there is a form, fit or function change of the application that is not backward compatible and that does not emulate the earlier product.
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